|  |  |
| --- | --- |
|  | CS 542 - Assignment 1 |
|  |  |
|  | Sukanta Sharma (A20472623), Vidya Sudarshan (A20472468), Vidhi Kakini (A20473969)  CS 542 – Computer Networks – I | Spring 2021 | Illinois Institute of Technology  4/1/21 |

1. What is the range of addresses that can assign to users in the 2021 block of class C? (3 points)

Ans:

Class C addresses start with to with the first 3 bytes as Net Id and the last byte as Host Id. As the block number starts with 0, so the 2021st block will be to be added to the first block of class C.

## 2021st Block:

To find the first address of the 2021st block, we need to add to the Net Id of the first address of the class C in base-256 number system.

**Converting**  **to base-256:**

| **Divisor** | **Dividend** | **Quotient** | **Remainder** |
| --- | --- | --- | --- |
| 256 | 2020 | 7 | 228 |
| 256 | 228 | 0 | 7 |

Therefore, 🡪

To get the range of the addresses in the 2021st block class C, we must find the first and the last address of the given block.

## First Address:

To find the first address of the 2021st block, we need to add with the Net Id .

| **+/-** | **Byte4** | **Byte3** | **Byte2** |
| --- | --- | --- | --- |
|  | 192 | 0 | 0 |
| + |  | 7 | 228 |
| **Result** | **192** | **7** | **228** |

With Net ID followed by zeros (0 bits), we can find the first address in the 2021st block as .

## Last Address:

As this is a class C address and the number of Host Id bits is 8, so each block will have addresses. To find the last address of the 2021st block, we need to add to the first address of the block.

| **+/-** | **Byte4** | **Byte3** | **Byte2** | **Byte1** |
| --- | --- | --- | --- | --- |
|  | 192 | 7 | 228 | 0 |
| + |  |  |  | 255 |
| **Result** | **192** | **7** | **228** | **255** |

So, the last address in the 2021st block as .

The range of addresses that can assign to users in the 2021st block of class C is .

1. Convert the number C0514019 in the hexadecimal base to the dotted-decimal notation. What is the class of this address? (consider classful addressing). (5 points)

Ans:

* Hexadecimal is a base-16 numerical system. It uses 16 distinct symbols to represent the value from 0 to 9, and to represent the value from 10 – 15. Here we will be considering per 2 digits of the hexadecimal to be equivalent to 1 byte in dotted-decimal notation and convert it to base-256 by each byte.

| **Hexadecimal** | **Conversion** | **Base-256 System** |
| --- | --- | --- |
|  |  |  |
|  | 5 |  |
|  | 4 |  |
|  | 1 |  |

The equivalent number of in dotted-decimal notation is **.**

1. Define the 1202 block of class B? (Give first and last address in the block) (3 points)

Ans:

Class B addresses start with to with the first 2 bytes as Net Id and the last 2 bytes as Host Id. As the block number starts with 0, so the 1202nd block will be to be added to the first block of class B.

## 1202nd Block:

To find the first address of the 1202nd block, we need to add to the Net Id of the first address of the class B in base-256 number system.

**Converting**  **to base-256:**

| **Divisor** | **Dividend** | **Quotient** | **Remainder** |
| --- | --- | --- | --- |
| 256 | 2020 | 7 | 228 |
| 256 | 228 | 0 | 7 |

Therefore, 🡪

To get the range of the addresses in the 1202nd block class B, we must find the first and the last address of the given block.

## First Address:

To find the first address of the 1202nd block, we need to add with the Net Id .

| **+/-** | **Byte4** | **Byte3** |
| --- | --- | --- |
|  | 128 | 0 |
| + | 4 | 177 |
| **Result** | **132** | **177** |

With Net ID followed by zeros (0 bits), we can find the first address in the 1202nd block as .

## Last Address:

As this is a class B address and the number of Host Id bits is 16, so each block will have addresses. To find the last address of the 1202nd block, we need to add to the first address of the block (i.e., ).

| **+/-** | **Byte4** | **Byte3** | **Byte2** | **Byte1** |
| --- | --- | --- | --- | --- |
|  | 132 | 177 | 0 | 0 |
| + |  |  | 255 | 255 |
| **Result** | **132** | **177** | **255** | **255** |

So, the last address in the 1202nd block as .

The range of addresses that can assign to users in the 1202nd block of class B is .

1. Convert the decimal number 5141.01568603515625 to the base 256 number system. (5 points)

Ans:

To convert to base-256 number system, we need to convert the integer part and the fraction part separately to base-256 and then we can combine them to obtain the result.

## Integer Part 🡪 :

| **Divisor** | **Dividend** | **Quotient** | **Remainder** |
| --- | --- | --- | --- |
| 256 | 5141 | 20 | 21 |
| 256 | 20 | 0 | 20 |

Therefore, 🡪

## Fraction Part 🡪 :

| **Multiplicand** | **Multiplier** | **Result** | **Integer Part** |
| --- | --- | --- | --- |
| 0.015686035 | 256 | 4.015625 | 4 |
| 0.015625 | 256 | 4 | 4 |

Therefore, 🡪 *[“,” is used as decimal point notation and “.” as separator of base-256 digits]*

Now, concatenating both the result we can write, 🡪 *[“,” is used as decimal point notation and “.” as separator of base-256 digits]*

1. What is the value of ? Give results in 256 base system. (Given numbers are in 256 base system) (4 points)

Ans:

## Conversion of to base-256 number system:

| **Divisor** | **Dividend** | **Quotient** | **Remainder** |
| --- | --- | --- | --- |
| 256 | 768 | 3 | 0 |
| 256 | 3 | 0 | 3 |

Therefore, is equivalent to

1. An organization is granted the block 142.200.208.0/21. The administrator wants to create 16 subnets.
2. Find the subnet mask (1 point).

Ans:

1. Find the number of addresses in each subnet (1 point)

Ans:

1. Find the subnet address and the direct broadcast address for the first subnet. (2 points)

Ans:

1. Find the 4th and 99th addresses in the last subnet. (4 points)

Ans:

1. Give the mask in the dotted-decimal notation:
2. For a block of Class-A which results in 128 subnets (1 point)

Ans:

1. Which combines 128 blocks of Class C into a supernet (1 point)

Ans:

1. Convert an IP address 256.128.64.32 to the binary notation (2 points)

Ans:

1. The 14th address of a block assigned to a specific organization is 120.65.89.141. The organization needs 120 addresses to give to its 120 users. Find the mask and define this block of addresses. Is there any wastage of the IP addresses? If yes, how many? (Note: The number of router interfaces is 2) (4 points)

Ans:

1. A block of addresses 120.200.240.0/20 granted to an ISP. These addresses are allocated between two groups of customers. The first group has 20 customers, each of which needs 64 addresses, the second group has 20 customers, each of which needs 128 addresses. Show the subblocks and range of addresses for the 10th customer of the first group and the 10th customer of the second group. How many addresses are still available after this allocation? (5 points)

Ans:

1. Find first address, last address, and number of addresses in the block, if one of the addresses in a block is 140.240.90.25/20 (3 points)

Ans:

1. Consider the following routing table (the next-hop address is omitted):

| **Mask** | **Network Address** | **Interface** |
| --- | --- | --- |
| /27 | 144.56.55.0 | M0 |
| /26 | 123.80.97.0 | M1 |
| /25 | 123.80.97.128 | M2 |
| /24 | 118.114.132.0 | M3 |
| Default | Default | M4 |

1. 144.56.55.31 (1 point)

Ans:

1. 144.56.56.31 (1 point)

Ans:

1. 123.80.97.60 (1 point)

Ans:

1. 123.80.97.200 (1 point)

Ans:

1. 123.80.97.88 (1 point)

Ans:

1. 118.114.133.1 (1 point)

Ans:

1. The routing table of routers R1, R2, and R3 are given. Draw the possible network configuration with all 3 routers, not separate configurations corresponding to each routing table. Indicate the next-hop addresses in the figure. (10 points)

R1:

| **Mask** | **Network Address** | **Next-Hop Address** | **Interface Number** |
| --- | --- | --- | --- |
| /24 | 80.70.56.0 | 100.160.32.67 | M2 |
| /24 | 130.135.7.0 | 150.137.45.78 | M1 |
| /16 | 180.170.0.0 | ----------------- | M0 |
| /16 | 100.160.0.0 | ----------------- | M2 |
| /16 | 150.137.0.0 | ----------------- | M1 |
| Default | Default | 180.170.4.6 | M0 |

R2:

| **Mask** | **Network Address** | **Next-Hop Address** | **Interface Number** |
| --- | --- | --- | --- |
| /24 | 80.70.56.0 | ----------------- | M0 |
| /16 | 100.160.0.0 | ----------------- | M1 |
| Default | Default | 100.160.56.7 | M1 |

R3:

| **Mask** | **Network Address** | **Next-Hop Address** | **Interface Number** |
| --- | --- | --- | --- |
| /24 | 130.135.7.0 | ----------------- | M0 |
| /16 | 150.137.0.0 | ----------------- | M1 |
| Default | Default | 150.137.72.48 | M1 |

Ans:

Considering the above routing tables for R1, R2, and R3, the possible network configuration diagram with all 3 routers is shown as below:




Figure 1: Network Diagram

1. Consider the network configuration below. A packet arrived at the router R3 with the destination address 150.14.8.56. Show how it is forwarded. (Assume classless addressing and mask of each network is /24) Create a routing table for R1 and R3. (10 points)



Ans: